int pin = 13; //this signifies which digital pin the power comes from

int pinP = 12;

void setup() {

// put your setup code here, to run once:

pinMode(pin, OUTPUT);

pinMode(pinP, OUTPUT);

}

void loop() {

// put your main code here, to run repeatedly:

digitalWrite(pin, LOW); //HIGH means on, LOW means off

delay(300);

digitalWrite(pin, HIGH);

digitalWrite(pinP, LOW);

delay(300);

digitalWrite(pinP, HIGH);

}